# CherryB Studio CB1800

![cb1800](https://i.imgur.com/QRJ6DFsl.jpg)

A G80-1800 inspired PCB for CB1800 Zakabato and any suitable 1800 layout keyboards.

* Keyboard Maintainer: [lunaticwhat](https://github.com/lunaticwhat)
* Hardware Supported: cb1800, atmega32u4
* Hardware Availability: [CherryB Studio](https://www.reddit.com/r/mechmarket/comments/mneayy/ic_cb1800zanbato_1800_classic_by_cherryb/)

Make example for this keyboard (after setting up your build environment):

    make cherrybstudio/cb1800:default

Flashing example for this keyboard:

    make cherrybstudio/cb1800:default:flash

## Accessing Bootloader Mode

To access Bootloader Mode, do one of the following:

* Tap the Reset switch mounted on the top side of the PCB to the left of the spacebar
* Hold the top left key of the keyboard while connecting the USB cable

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
