# CONSTELLATION REV2

A gasket 65% keyboard by [aeboards](https://aeboards.com/)

* Keyboard Maintainer: [Xelus22](https://github.com/Xelus22)
* Hardware Supported: CONSTELLATION
* Hardware Availability: Custom keyboard group buys

Make example for this keyboard (after setting up your build environment):

    make aeboards/constellation/rev2:default

Reset your keyboard in 3 ways:
<ol>
<li>Software reset on Fn + Backspace</li>
<li>Bootmagic reset: hold down the top left key (usually escape) and plugin the keyboard</li>
<li>Physical reset button: on the back of the PCB, there are 2 open pins which you can short, labelled RESET</li>
</ol>

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
