# AMJ60

![AMJ60](https://raw.githubusercontent.com/noroadsleft/qmk_images/master/keyboards/amj60/s-l1200_640.jpg)

A 60% keyboard.

* Keyboard Maintainer: [The QMK Community](https://github.com/qmk)
* Hardware Supported: AMJ60
* Hardware Availability: [~~Taobao~~](http://item.taobao.com/item.htm?id=43500549469) (no longer available)
* References: [Geekhack](https://geekhack.org/index.php?topic=77636.0)

Make example for this keyboard (after setting up your build environment):

    make amjkeyboard/amj60:default

Flashing example for this keyboard:

    make amjkeyboard/amj60:default:flash

To reset the board into bootloader mode, tap the Reset switch mounted on the bottom side of the PCB.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
