# GH60 v1.3

![GH60 v1.3](https://raw.githubusercontent.com/noroadsleft/qmk_images/master/keyboards/gh60/v1p3/pcb_bottom.jpg)

A 60% with USB Type-C, in-switch backlight, and RGB Underglow. Also called GH60 RGB.

* Keyboard Maintainer: [The QMK Community](https://github.com/qmk)
* Hardware Supported: GH60 V1.3 PCB, ATmega32U4
* Hardware Availability: [NPKC RGB CP Store on AliExpress](https://www.aliexpress.com/i/32851321035.html)

Make example for this keyboard (after setting up your build environment):

    make gh60/v1p3:default

Flashing example for this keyboard:

    make gh60/v1p3:default:flash

## Layouts

[Reference Image](https://raw.githubusercontent.com/noroadsleft/qmk_images/master/keyboards/gh60/v1p3/layouts.jpg)

The `factory_*` keymaps are based on KBFirmware JSON files provided by the vendor. Layouts 1 (Minila), 3 (Poker), 5, 7, 9, and HHKB (not pictured) have keymaps present.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
