# Drashna's Blackpill Tractyl Manuform (5x6) with a right side trackball


* Split Hand Pin, using PC14
* Full Duplex Serial/USART using PA9 and PA10 on USART1
* DAC Audio using PA4 and PA5
* PWM RGB using PA6 TIM3
* pmw3360 sensor using PA5-PA7 on SPI2, with B as CS pin
* 8KB SPI EEPROM chip sharing PB13-PB15 on SPI1 with PB9 as CS pin
* Encoder using PA7 and PA8
* SSD1306 OLED display (128x64) using PB6 and PB7 on I2C1

* Keyboard Maintainer: [Drashna Jael're](https://github.com/drashna)
* Hardware Supported: [Design files](https://gitlab.com/keyboards1/dm_r_track/-/tree/master/boolean), [WeAct BlackPill (F411)](https://github.com/WeActStudio/WeActStudio.MiniSTM32F4x1), [PMW3360 Optical Sensor](https://www.tindie.com/products/jkicklighter/pmw3360-motion-sensor/)

Make example for this keyboard (after setting up your build environment):

    make handwired/tractyl_manuform/5x6_right/f411:default

Flashing example for this keyboard:

    make handwired/tractyl_manuform/5x6_right/f411:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
