# PaladinPad PCB

Firmware for the PaladinPad, with underglow.

* Keyboard Maintainer: [KapCave](https://github.com/nachie)
* Hardware Supported: PaladinPad
* Hardware Availability: [KapCave](https://kapcave.com/products/paladinpad-pcb)

Make example for this keyboard (after setting up your build environment):

    make kapcave/paladinpad:default

Or to make and flash:

    make kapcave/paladinpad:default:flash


See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Bootloader

* **Bootmagic reset**: Hold down NumLock (Top Left) and plug in the keyboard
* **Physical reset button**: Briefly press the button labeled "SW_RST1" on the back of the PCB
