# Bubble 75

![image](https://i.imgur.com/9J01bYHh.png)


A compact exploded F-Row 75% made by Velocifire.

* Keyboard Maintainer: [d-floe](https://github.com/d-floe)
* Hardware Supported: Bubble75 Hotswap
* Hardware Availability: [velocifiretech.com](https://www.velocifiretech.com/collections/keyboards/products/bubble-75-premium-keyboard-kit?variant=39743137939574)

Make example for this keyboard (after setting up your build environment):

    make bubble75/hotswap:default

Flashing example for this keyboard:

    make bubble75/hotswap:default:flash
    
Bootloader: Press the physical reset button on the bottom side of the PCB or hold down ESC while plugging in the board.
    
See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
