# Axon40

The Axon40 PCB is a modified layout for the Neuron ortho. It's ortho but with a bottom row with larger than 1u keys. 

- Keyboard Maintainer: Nasp
- Hardware Supported: Axon40
- Hardware Availability: www.CheckerBoards.xyz

Make example for this keyboard (after setting up your build environment):

    make checkerboards/axon40:default

Enter the bootloader by shorting GND and RESET between switches 37 and 38.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
