# 3dp660

![](https://i.imgur.com/KWyU57el.jpg)

### Teensy 2.0 Pinout
| rows            | 0   | 1   | 2   | 3   | 4   |
| --------------- | --- | --- | --- | --- | --- |
| Teensy/QMK pin  | B0  | B1  | B2  | B3  | B7  |

| columns         | 0   | 1   | 2   | 3   | 4   | 5   | 6   | 7   | 8   | 9   | 10  | 11  | 12  | 13  | 14  |
| --------------- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Teensy/QMK pin  | D2  | D3  | C6  | C7  | D5  | D4  | D7  | B4  | B5  | B6  | F7  | F6  | F5  | F4  | F1  |


Make example for this keyboard (after setting up your build environment):

    make handwired/3dp660:default

**Reset Key:** Hold down the key located at `k00`, commonly programmed as Escape while plugging in the keyboard.

* Keyboard Maintainer: [gooberpsycho](https://github.com/gooberpsycho)
* Hardware Availability: [Casefile](https://www.thingiverse.com/thing:2897260)

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
