# Adafruit KB2040 onekey with OLED

To trigger keypress, short together pins *GP4* and *GP5*.

Double-tap reset to enter bootloader mode. Copy the built uf2 file to the device by dragging the file to the new USB disk.

## Supported Hardware

* [Adafruit KB2040 - RP2040 Kee Boar](https://www.adafruit.com/product/5302)
* Optional [128x32 OLED display on the Stemma QT port](https://www.adafruit.com/product/4440)
