# GHS.JEM

![GHS.JEM](https://i.imgur.com/whcvQ01l.jpg)

A 65% screwless seamless keyboard.

* Keyboard Maintainer: [Ramon Imbao](https://github.com/ramonimbao)
* Hardware Supported: ATmega32u4
* Hardware Availability: [Gone Hacking Studio][https://gonehacking.studio/]

To access the bootloader, press the reset button located under the spacebar. You can then flash new firmware:

Make example for this keyboard (after setting up your build environment):

    make ghs/jem:default

Flashing example for this keyboard:

    make ghs/jem:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
