# CMM.Studio Saka68

CMM.Studio Saka68 Keyboard

![CMM.Studio Saka68](https://i.imgur.com/E1S43cs.png)




* Keyboard Maintainer: [CMM.Studio Freather](https://github.com/CMMS-Freather)
* Hardware Supported: PCB, Atmega32u4
this firmware supports iso and ansi hotswap directly, once you flash the via firmware, you only need to select the layout and change to iso layout, then you can use iso hotswap version

Make example for this keyboard (after setting up your build environment):

    make cmm_studio/saka68/hotswap:default


For reset instruction, use the physical reset button on the back of the keyboard to enter bootloader mode

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
