# Glacier

1800 Style Keyboard based on the Austin

* Keyboard Maintainer: Swiftrax
* Hardware Supported: Glacier
* Hardware Availability: Glacier PCB

## Bootloader Enter the bootloader in 3 ways:
 * **Bootmagic reset**: Hold down the key at (0,0) in the matrix (usually the top left key or Escape) and plug in the keyboard
 * **Physical reset button**: Briefly press the button on the back of the PCB - some may have pads you must short instead
 * **Keycode in layout**: Press the key mapped to `QK_BOOT` if it is available

Make example for flashing this keyboard (after setting up your build environment):

    make handwired/swiftrax/glacier:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
