# SCARLET

![scarlet](https://www.draytronics.co.uk/wp-content/uploads/2020/10/Scarlet-PCB-Compared-Combined.png)

A open source 17 key numpad keyboard, designed to be easily built at home with through hole components. More info / kits / PCB designs available at [draytronics.co.uk/scarlet](https://draytronics.co.uk)

* Keyboard Maintainer: [Blake Drayson](https://github.com/ghostseven)
* Hardware Supported: SCARLET PCB / ATMega32A
* Hardware Availability: [draytronics.co.uk](https://draytronics.co.uk)

Make example for this keyboard (after setting up your build environment):

    make draytronics/scarlet:default

Flashing example for this keyboard:

    make draytronics/scarlet:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

VIA design config file avaliable [here](https://www.draytronics.co.uk/f_scarlet/draytronics_scarlet_via_config.json)
