# IDOBAO ID87 v2

![IDOBAO ID87](https://i.imgur.com/LIpWjog.png)

A TKL hotswap board from IDOBAO.

## ANSI Support

* Keyboard Maintainer: [Vino Rodrigues](https://github.com/vinorodrigues)
* Hardware Supported:
  - **IDOBAO ID87v2**
  - **IDOBAO ID87 Crystal**
  - **IDOBAO ID87 Bestype**
  - **IDOBAO ID87 Charm** *(Limited Edition)*
* Hardware Availability: [IDOBAO.net](https://idobao.net/search?type=product&q=ID87*)

## ANSI Layout

![](https://idobao.github.io/kle/idobao-id87.png)

## Compiling & Flashing

Make example for this keyboard (after setting up your build environment):

    make idobao/id87/v2:default

Flashing example for this keyboard:

    make idobao/id87/v2:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Bootloader

Enter the bootloader in 3 ways:

* **Bootmagic reset**: Hold down the [Escape] key *(the top left)* and plug in the keyboard
* **Physical reset button**: Briefly press the button on the back of the PCB
* **Keycode in layout**: Press the key mapped to `QK_BOOT` *(default is [Fn]+[Escape])*
