# a65i

![a65i](https://i.imgur.com/J4fzVVth.jpg)

PCB designed by Lfgberg for the AnomalyKB a65i.

To enter bootloader mode, either utilize the reset button near the MCU, or short the ESC key for bootmagic lite.

* Keyboard Maintainer: [Lfgberg](https://github.com/lfgberg)
* Hardware Supported: A65I PCB
* Hardware Availability: [AnomalyKB](anomalykb.co)

Make example for this keyboard (after setting up your build environment):

    make anomalykb/a65i:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
