# handwired/dc/mc/001

[![handwired/dc/mc/001](https://i.imgur.com/bv2g32U.jpg)
*A freestanding media controller*](https://imgur.com/a/PM9lQ)

* Keyboard Maintainer: [Daniel Cormier](https://github.com/dcormier)
* Hardware Supported: Adafruit Atmega32u4 Breakout Board
* Hardware Availability: https://www.adafruit.com/product/296

Make example for this keyboard (after setting up your build environment):

    make handwired/dc/mc/001:default

Flashing example for this keyboard:

    make handwired/dc/mc/001:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Bootloader

Enter the bootloader:

* **Physical reset button**: Briefly press the button on the top of the PCB
