# CU7

The CU7 is a customisable 3x2 key macropad with a clickable rotary encoder.

To place the keyboard into bootloader mode in order to flash it, use the reset button on the PCB.

* Keyboard maintainer: [rys](https://github.com/rys)
* Hardware supported: CU7
* Hardware availability: [CapsUnlocked](https://caps-unlocked.com/cu7/)

Make and flash example for this keyboard (after setting up your build environment):

    make capsunlocked/cu7:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
