# Coban Pad 9A

![Coban Pad 9A](https://i.imgur.com/5svg1RMh.jpeg)

Small macro keyboard with 6 hotswapable button and 2 EC11 rotary encoder

* Keyboard Maintainer: [RyanDam](https://github.com/RyanDam)  
* Hardware Supported: Coban Pad 9A

Make example for this keyboard (after setting up your build environment):

    make coban/pad9a:default

Flashing example for this keyboard:

    make coban/pad9a:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Bootloader

Enter the bootloader:

* **boot button**: Hold the BOOT button on the back of the PCB while plug in usb cable
