# gorthage_truck

This PCB is a drop-in ortholinear replacement for the Garbage Truck keyboard case. It supports 2x3u split bars, 7u, or 10u.

* Keyboard Maintainer: [s8erdude](https://github.com/jpuerto96)
* Hardware Supported: Gorthage Truck PCB
* Hardware Availability: [Open Source PCB](https://github.com/jpuerto96/gorthage_truck)

Make example for this keyboard (after setting up your build environment):

    make gorthage_truck:default

Flashing example for this keyboard:

    make gorthage_truck:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

To reset the board, you will want to short the pad labeled RESET1 on the back (near the MCU).
