# Potato65 Solderable Keyboard

![Potato65 Solderable](https://i.imgur.com/ysAGZCmh.jpg)

A solderable gasket mount stacked acrylic 65% keyboard

-   Keyboard Maintainer: [Maelkk](https://github.com/Aeonstrife)
-   Hardware Supported: Potato65 Keyboard
-   Hardware Availability: Private Group-Buy

Make example for this keyboard (after setting up your build environment):

    make buildakb/potato65s:default

Flashing example for this keyboard:

    make buildakb/potato65s:default:flash

To reset into bootloader mode:

While plugged in, press the RESET switch located on the back of the pcb.
The keyboard should now be in bootloader mode.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).