# lemonpad

![lemonpad](https://i.imgur.com/hAp2Nich.jpeg)

This is a QMK and VIA implementation for an atmega32u4 based adaptation of the Adafruit Lemon Keypad. By default it uses a Pro Micro, if you would like to use a different microcontroller please make sure you have the correct bootloader set. 

* Keyboard Maintainer: [dari-studios](https://github.com/dari-studios)
* Hardware Supported: atmega32u4 based boards with the Caterina bootloader
* Hardware Availability: https://learn.adafruit.com/qtpy-lemon-mechanical-keypad-macropad

Make example for this keyboard (after setting up your build environment):

    make handwired/lemonpad:default

Flashing example for this keyboard:

    make handwired/lemonpad:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Bootloader

Enter the bootloader in 3 ways:

* **Bootmagic reset**: Hold down the key at (0,0) in the matrix (usually the top left key or Escape) and plug in the keyboard
* **Physical reset button**: Briefly press the button on the back of the PCB - some may have pads you must short instead
* **Keycode in layout**: Press the key mapped to `QK_BOOT` if it is available
