# Quark_LP

![Quark_LP](https://i.imgur.com/EgdbzxE.png)

The Quark LP PCB is compatible with Cherry Low-Profile switches and Kailh Choc switches, and is drop-in compatible with the OLKB Planck board. 

* Keyboard Maintainer: [Nasp](https://github.com/npspears)
* Hardware Supported: Planck
* Hardware Availability: www.checkerboards.xyz

Make example for this keyboard (after setting up your build environment):

    make checkerboards/quark_lp:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Bootloader
Enter the bootloader by pressing the reset pin on the back of the PCB. You can do this through the back of the case through the small hole near the USB connector. 
