# Default VIA Keymap
Compile the firmware with this keymap for use the BMEK with the [VIA configurator](https://caniusevia.com/).
Layout options can be configured in VIA (see first screenshot below).

## 0: Base Layer
![Base Layer](https://i.imgur.com/tBu50SS.png)

## 1: Nav Layer
![Nav Layer](https://i.imgur.com/ZzEow3t.png)

## 2: NUM Block
![NUM Block](https://i.imgur.com/vzjZIa1.png)

## 4: FW Config
![FW Config](https://i.imgur.com/L7QynAb.png)

## Alternative Preconfigured Layouts
TODO: Provide (links to) some alternative via keymaps after VIA support is landed upstream.
