# KabeDon 98e

![KabeDon98e](https://gitee.com/kabedon/picture/raw/master/pictures/980e.jpg)

A mechanical keyboard PCB similar to 980 layout, it has two encoders.
This PCB uses kailh hot swap socket.
Kabedon980 includes RGB underflow.

* Keyboard Maintainer: [370490639](https://github.com/370490639)
* Hardware Supported: f103 KabeDon98e
* Hardware Availability: [KabeDon98e]https://kabedon.taobao.com

Make example for this keyboard (after setting up your build environment):

    make kabedon/kabedon98e:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
