# IDOBAO Montex V2

![MONTEX V2](https://i.imgur.com/uHEispxh.png)

A hotswap RGB numpad from IDOBAO.


## Numeric Keypad

* Keyboard Maintainer:
    - [IBNobody](https://github.com/IBNobody)
    - [vinorodrigues](https://github.com/vinorodrigues)
* Hardware Supported: **IDOBAO Montex V2**
* Hardware Availability: [IDOBAO.net](https://idobao.net/search?type=product&q=montex*)


## Layout

![](https://idobao.github.io/kle/idobao-id27-v2.png)


## Compiling and Flashing

Make example for this keyboard (after setting up your build environment):

    make idobao/montex/v2:default

Flashing example for this keyboard:

    make idobao/montex/v2:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information.<br>
Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Bootloader

Enter the bootloader in 3 ways:

* **Bootmagic reset**: Hold down the key at (0,0) in the matrix (usually the top left key or Escape) and plug in the keyboard
* **Physical reset button**: Briefly press the button on the back of the PCB
* **Keycode in layout**: Press the key mapped to `QK_BOOT` if it is available
