# KD87A_BFG_Edition 
![KD87A_BFG_Edition](https://imgur.com/uOUvWvwh.png)

An 87 keys keyboard, Equipped with the WestBerry Q95 microcontroller.

* Keyboard Maintainer: [GSKY](https://github.com/gksygithub)
* Hardware Supported: KD87A_BFG_Edition
* Hardware Availability: [GSKY GitHub](https://github.com/gksygithub/keyboard1)

Make example for this keyboard (after setting up your build environment):

    make darkproject/kd87a_bfg_edition:default

Flashing example for this keyboard:

    make darkproject/kd87a_bfg_edition:default:flash

To reset the board into bootloader mode, do one of the following:

* Hold the Reset switch mounted on the surface of the PCB back side after the USB cable is connected
* Hold the Escape key while connecting the USB cable (also erases persistent settings)
* Fn+ESC will reset the board to bootloader mode

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
