# osborne1

![osborne1](https://i.imgur.com/221nQ5Eh.jpeg)

The Osborne keyboard doesn't contain any electronics, so the pins of the 8x8 keyboard matrix are easily available right on the normal connector. 17 jumper wires and a Feather BlueFruit is all the additional hardware needed.

* Keyboard Maintainer: [crackmonkey](https://github.com/crackmonkey)
* Hardware Supported: Adafruit Feather BlueFruit 32u4
* Hardware Availability: E-waste

Make example for this keyboard (after setting up your build environment):

    make osborne1:default

Flashing example for this keyboard:

    make osborne1:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Bootloader

Enter the bootloader:

* **Physical reset button**: Briefly press the button on the Feather
