# Ready100

The following is the QMK Firmware for the [Ready100](https://www.ready100.com) 64-key PCB, a universal tray mount 60% hotswap PCB with per key RGB LED's. 

The PCB will feature:
* Kailh Hotswap sockets
* QMK & VIA compatibility
* Per-Key RGB LED's

---

* Keyboard Maintainer: FJLabs
* Hardware Supported: Ready100

Make example for this keyboard (after setting up your build environment):

    make fjlabs/ready100:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs). You can enter the bootloader by pressing the reset button on the back of the PCB.
