# MutePad

[MutePad Repo](https://github.com/JoshwJB/MutePad)

A 3D printed under desk mounted keypad with rotary encoder, for muting applications (discord, zoom etc.) and adjusting volume.

* Keyboard Maintainer: [JoshwJB](https://github.com/JoshwJB)
* Hardware Supported: ProMicro
* Hardware Availability: Handwired - see [MutePad Repo](https://github.com/JoshwJB/MutePad)

Make example for this keyboard (after setting up your build environment):

    make handwired/mutepad:default

Flashing example for this keyboard:

    make handwired/mutepad:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Bootloader

Enter the bootloader in 2 ways:

* **Bootmagic reset**: Hold down the key at (0,0) in the matrix (usually the top left key or Escape) and plug in the keyboard
* **Physical reset button**: Briefly short the ground and reset on the ProMicro

## Images
![image](https://user-images.githubusercontent.com/15612025/157335123-a76ce059-86b4-4484-9bb2-0abff8a13cc8.png)

### Wiring
![image](https://user-images.githubusercontent.com/15612025/157336673-ad348e3d-4314-4703-afe0-a43a6f73b892.png)
![image](https://user-images.githubusercontent.com/15612025/157335150-8491553f-a7dc-462a-a6af-bc4be223b703.png)
