# Potato65

![Potato65](https://i.imgur.com/DAxaygo.jpg)

A simple 65% pcb with underglow. Compatible with most TADA68 cases.

-   Keyboard Maintainer: [Maelkk](https://github.com/Aeonstrife)
-   Hardware Supported: Potato65 PCBs
-   Hardware Availability: Private Group-Buy

Make example for this keyboard (after setting up your build environment):

    make buildakb/potato65:default

Flashing example for this keyboard:

    make buildakb/potato65:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
