# Jels60

![jels60](https://i.imgur.com/3Ec4YZNh.png)

A 60% PCB

* Keyboard Maintainer: [Jels](https://github.com/Jels02)
* Hardware Supported: Jels60 PCB
* Hardware Availabililty: Limited Group buys

Make example for this keyboard (after setting up your build environment):

    make jels/jels60:default

Flashing example for this keyboard:

    make jels/jels60:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

* **Bootmagic reset**: Hold down the top left key (ESC/Tilde) and plug in the keyboard
* **Physical reset button**: Briefly press the button on the back of the PCB
* **Keycode in layout**: Press the key mapped to `QK_BOOT` if it is available
