# Emi20

![Emi20](https://i.imgur.com/Mc84fLGl.jpg)

A compact 4x5 ortholinear keyboard made by Project Aqua and sold by Evil-cables.

* Keyboard Maintainer: [AquaCylinder](https://github.com/AquaCylinder)
* Hardware Supported: PCB, Atmega32u4
* Connector: USB mini B

Make example for this keyboard (after setting up your build environment):

    make emi20:default

To reset the board into bootloader mode, press the physical reset button on the back of the PCB or press the bottom most left key to momentarily switch to layer 2 (on layer 1) and then press the key from the top right down one.

The default keymap.c file has comments to help you on your journey,
See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
