# CherryB Studio CB87

![CB87](https://i.imgur.com/balJ20Xl.png)

A TKL PCB for CherryB Studio Freyr and replacement for some TKL keyboards.

* Keyboard Maintainer: duongaanh
* Hardware Supported: CB87, atmega32u4
* Hardware Availability: [CherryB Studio](https://www.reddit.com/r/mechmarket/comments/kkgs6p/gb_freyr_tkl_cb_edition_holiday_preorder/)

Make example for this keyboard (after setting up your build environment):

    make cherrybstudio/cb87:default

Flashing example for this keyboard:

    make cherrybstudio/cb87:default:flash

## Accessing Bootloader Mode

To access Bootloader Mode, do one of the following:

* Tap the Reset switch mounted on the top side of the PCB to the left of the spacebar
* Hold the top left key of the keyboard while connecting the USB cable

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
