# Hydrogen Deskpad

A 5 key macropad with an encoder, that can be mounted to a desk or below your monitor.

* Keyboard Maintainer: [Hydrogen BD](https://www.facebook.com/hgenbd/)
* Hardware Supported: [5k Deskpad](https://fb.watch/akRLW7s-UT/)

Make example for this keyboard (after setting up your build environment):

    make h0oni/deskpad:default

## Bootloader

Enter the bootloader in 2 ways:

* **Bootmagic reset**: Hold down the key at (0,0) in the matrix (the left most key) and plug in the keyboard.
* **Physical reset button**: Press the button at the back of the PCB twice to enter into the bootloader mode. 

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).