# Raspberry Pi 2040 onekey

To trigger keypress, short together pins *GP4* and *GP5*.

Double-tap reset to enter bootloader mode. Copy the built uf2 file to the device by dragging the file to the new USB disk.

## Supported Hardware

* Raspberry Pi Pico
* SparkFun Pro Micro - RP2040
* Adafruit KB2040 - RP2040 Kee Boar
* ...and many more RP2040 based development boards
