# CherryB Studio CB87v2

![cb87v2](https://i.imgur.com/0DqZDXw.jpg)

An advance TKL PCB with many configurable layouts

* Keyboard Maintainer: [lunaticwhat](https://github.com/lunaticwhat)
* Hardware Supported: cb87v2, atmega32u4
* Hardware Availability: [CherryB Studio](https://discord.gg/qVwv3gcq83)

Make example for this keyboard (after setting up your build environment):

    make cherrybstudio/cb87v2:default

Flashing example for this keyboard:

    make cherrybstudio/cb87v2:default:flash

## Accessing Bootloader Mode

To access Bootloader Mode, do one of the following:

* Tap the Reset switch behind the PCB near the MCU
* Hold the top left key of the keyboard while connecting the USB cable

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
