# USB C Model M

![modelm_usbc](https://raw.githubusercontent.com/ashpil/Model-M-Type-C-Controller/master/images/render.png)

This is a configuration of QMK intended to be used with the [USB C Model M alt controller](https://github.com/ashpil/Model-M-Type-C-Controller "USB C Model M alt controller"). Many thanks to iw0rm3r for working on a similar project and providing the foundation for this!

* Keyboard Maintainer: [ashpil](https://github.com/ashpil)
* Hardware Supported: [USB C Model M alt controller](https://github.com/ashpil/Model-M-Type-C-Controller)

Make example for this keyboard (after setting up your build environment):

    make ibm/model_m/ashpil_usbc:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
