# Budget96

A budget-oriented 96 key atmega32a keyboard. Runs ps2avrgb by default.  

* Keyboard Maintainer: [MechMerlin](https://github.com/mechmerlin), [DonutCables](https://github.com/DonutCables)
* Hardware Supported: Budget96 PCB
* Hardware Availability: [DonutCables](https://donutcables.com/)

Make example for this keyboard (after setting up your build environment):

    make donutcables/budget96:default

Flashing example for this keyboard ([after setting up the bootloadHID flashing environment](https://docs.qmk.fm/#/flashing_bootloadhid))

    make donutcables/budget96:default:flash

**Reset Key**: Hold down the key located at *K00*, commonly programmed as *left control* while plugging in the keyboard.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
