# CMM.Studio Saka68

CMM.Studio Saka68 Keyboard

![CMM.Studio Saka68](https://i.imgur.com/gZ9Thjel.png)

* Keyboard Maintainer: [CMM.Studio Freather](https://github.com/CMMS-Freather)
* Hardware Supported: PCB, Atmega32u4

Make example for this keyboard (after setting up your build environment):

    make cmm_studio/saka68/solder:default


For reset instruction, use the physical reset button on the back of the keyboard to enter bootloader mode

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
