# Swift65

A 65% Keyboard from Swiftcables

* Keyboard Maintainer: [Steven Phillips (spooknik)](https://github.com/keyboardcollective)
* Hardware Supported: Swift65 Hotswap
* Hardware Availability: Soom from Swiftcables

To enter bootloader for flashing firmware, press layer change key (MO(1)) and Right Shift simultaneously.

Make example for this keyboard (after setting up your build environment):

    make alfredslab/swift65/hotswap:default

Flashing example for this keyboard:

    make alfredslab/swift65/hotswap:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
