# BINEPAD BN009

![BINEPAD BN009](https://imgur.com/fu0iXD0h.jpg)

A 9% macropad.

* Keyboard Maintainer: [binepad](https://github.com/binepad)
* Hardware Supported:
    * BN009 R1 *(ft. ATmega32U4)*
    * BN009 R2 *(ft. STM32F103)*
* Hardware Availability: [binepad.com](https://www.binepad.com/bn009)

Make example for this keyboard (after setting up your build environment):

    make binepad/bn009/r1:default

..or..

    make binepad/bn009/r2:default

Flashing example for this keyboard:

    make binepad/bn009/r1:default:flash

..or..

    make binepad/bn009/r2:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information.
Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Bootloader

Enter the bootloader in 3 ways:

* **Bootmagic reset**: Hold down the key at (0,0) in the matrix (usually the top left key) and plug in the keyboard
* **Physical reset button**: Briefly press the button under the small hole on the back of the macropad
* **Keycode in layout**: Press the key mapped to `QK_BOOT` or `RESET` if it is available
