# Default keymap for the vim clutch

The two enclosure tactile switches change between modes "voice chat" (default) and "vim clutch."

The voice chat mode uses `F13` to activate or deactivate push-to-talk.

The vim clutch uses the `ESC` and `a` keys to clutch into and out of vim.
