# AMJ40

![AMJ40](https://raw.githubusercontent.com/noroadsleft/qmk_images/master/keyboards/amj40/AMJ40-Keyboard-Side-scaled_640.jpg)\
[PCB photo](https://raw.githubusercontent.com/noroadsleft/qmk_images/master/keyboards/amj40/DSC_1718-768x512_640)

DIY/Assembled compact 40% keyboard.

* Keyboard Maintainer: QMK Community
* Hardware Supported: AMJ40 PCB
* Hardware Availability: no longer available
* References: [Flashquark](https://flashquark.com/product/amj40-40-mechanical-keyboard-kit/), [geekhack](https://geekhack.org/index.php?topic=87961.0)

Make example for this keyboard (after setting up your build environment):

    make amjkeyboard/amj40:default

Flashing example for this keyboard:

    make amjkeyboard/amj40:default:flash

To reset the board into bootloader mode, hold the key at the top left of the keyboard while connecting the USB cable (also erases persistent settings).

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
