# jk01 

An 83 keys keyboard, Equipped with the WestBerry Q95 microcontroller.

* Keyboard Maintainer: [JUKAIE](https://github.com/jukaie)
* Hardware Supported: JK01
* Hardware Availability: [JUKAIE](https://github.com/jukaie/keyboard1)

Make example for this keyboard (after setting up your build environment):

    make jukaie/jk01:default

Flashing example for this keyboard:

    make jukaie/jk01:default:flash

To reset the board into bootloader mode, do one of the following:

* Hold the Reset switch mounted on the surface of the PCB back side after the USB cable is connected
* Hold the Escape key while connecting the USB cable (also erases persistent settings)
* Fn+ESC will reset the board to bootloader mode

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
