# The default keymap for Panda65_01

![Panda65_01 layout image](https://i.imgur.com/fPBUDMT.png)

* Keyboard Maintainer: [generic_panda](https://github.com/jesseleung97)
* Hardware Supported: panda65_01 PCB
* Hardware Availability: [panda65-01 acrylic case designed by Alec:](https://onedrive.live.com/?authkey=%21AA8d6frZ0woiaV4&id=DC069E9FB0BC8004%21155830&cid=DC069E9FB0BC8004) 

Make example for this keyboard's default keymap (after setting up your build environment):

    make generic_panda/panda65_01:default

Flashing example for this keyboard:

    make generic_panda/panda65_01:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
