# Jones

![Jones, "Wide" layout](https://raw.githubusercontent.com/jpskenn/Jones/master/assets/_DSF0714.jpeg)

A symmetrical 60% keyboard combined with Ortho-Linear and Row-staggered. It has gapless Row 2 - Row 3.  
GH60 case compatible PCB and keyplate.  
[More info](https://github.com/jpskenn/Jones)

* Keyboard Maintainer: [jpskenn](https://github.com/jpskenn)
* Hardware Supported: PCB, Key plate, Bottom plate
* Hardware Availability: [GitHub](https://github.com/jpskenn/Jones), [BOOTH](https://jpskenn.booth.pm), [Yushakobo](https://yushakobo.jp)

Make example for this keyboard (after setting up your build environment):

    make jones/v1:default

Flashing example for this keyboard ([using the command line](https://docs.qmk.fm/#/newbs_flashing?id=flash-your-keyboard-from-the-command-line)):

    make jones/v1:default:flash

To reset the keyboard into bootloader mode, press the reset switch on the underside.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
