# hnah108

![hnah108](https://i.imgur.com/rV0lM8Ml.jpg)

A full size keyboard pcb with rotary encoder. Uses WS2811 IC as an indicator LED driver.

* Keyboard Maintainer: [HnahKB](https://github.com/vuhopkep)
* Hardware Supported: Hnah108 v1

Make example for this keyboard (after setting up your build environment):

    make handwired/hnah108:default

Flashing example for this keyboard:

    make handwired/hnah108:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
