TA-65
=====

A 65% PCB designed to fit the TADA68, Kayak and others by [Evyd13](https://github.com/evyd13).

![kle](https://maartenwut.com/wp-content/uploads/2019/02/ta-65-layouts-768x420.png)

Keyboard Maintainer: QMK Community<br>
Hardware Supported: TA-65 PCB<br>
Hardware Availability: [maartenwut.com](https://maartenwut.com/product/ta-65/)<br>

Make example for this keyboard (after setting up your build environment):

    make ta65:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

