# Wasdat

![wasdat](https://maartenwut.com/wp-content/uploads/2019/02/by72xkc5-600x600.jpg)

A drop-in replacement controller for the WASD v2 TKL and fullsize models.

* Keyboard Maintainer: [Evyd13](https://github.com/evyd13)
* Hardware Supported: WASD v2 TKL/Fullsize ANSI & ISO with Wasdat controller
* Hardware Availability: [maartenwut.com](https://maartenwut.com/product/wasdat/)

## Flashing

The WASD has no reset button, but it does have a bank of DIP switches on the bottom, so to enter the bootloader on this board, simply toggle the first one on and off.

---

Make example for this keyboard (after setting up your build environment):

    make evyd13/wasdat:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
